**Proposed revision to III.D.7 of the Harbor 20 Class Bylaws**

The rudder shall not be altered in any way from its original shape as designed and molded. A builder supplied rudder head, or its equivalent is required. The rudder post and sleeve in the hull of the boat will not be modified from the original design. Bearings are not allowed.

The dimensions and shape of the rudder are as follows.

The critical dimensions are: depth 31.50 inches +/- .25 inches when measured along the trailing edge from top to bottom; fore-and-aft distance at the top is 15.30 inches +/- .20 inches; fore-and-aft distance at a point 3 inches above the bottom is 9.0 inches +/- .20 inches.

The leading edge will be a smooth radius as developed in the mold.

The trailing edge will be a flat surface .25 inches wide +/- .06 inches.